# Push-Pull Snubber

Transformer leakage inductance | LT = |  | µH
Schottky junction capacitance | CJ = |  | pF
Primary to secondary turns ratio | n = |  | NP/NS
Snubber capacitance (10nF - 100nF) | CS = |  | nF
Switching frequency | FS = |  | kHz
Input voltage | VIN = |  | V
Calculate RS |  |
Snubber resistance | RS = |  | Ohm
Power dissipated in RS | PR = |  | mW
Reset form |  |  |  |

Source:High frequency Switching Power Supplies, George Chryssis