# Calculate reverse recovery diode model parameters

Maximum current during conduction | IF = |  | A
Maximum Reverse Recovery current | IRM = |  | A
Reverse saturation current | IS = |  | A
Emission coeffficient (default=1 power diodes=2) | N = |  |
Forward conduction interval | T0 = |  | s
Reverse conduction interval | T1 = |  | s
Reverse recovery time constant | taurr = |  | s
Calculate reverse recovery parameters |  |
Reverse saturation current | IS = |  | A
Time interval | TM = |  | us
Reverse recovery time constant | tau = |  | us
Model name | ModelName = |  |
.Model | Model = |  |
Write results to .model file |  |  |  |
Reset form |  |  |  |